# Revision History

| **Date** | **Version** | **Revision** |
| --- | --- | --- |
|  |  |  |
| 2016/10/20 | 6.01.01.18 | 1. Fixed the bug: Wave trace departs from zero line while there is offset 2. Fixed the bug: Sample rate of zoom changed after STOP in dot display mode 3. Fixed the bug: All measurements are on, select source on a disable channel. Reboot the Scope, then the software hang on the boot screen 4. Adjusted keyboard scan method to optimize recognizing keyboard value 5. Modified BMP from 24 bit to 16 bit while save/get BMP form Scope |
| 2015/11/30 | 6.01.01.08 | The first formal release |
|  |  |  |

# Compatibility between Versions

| **Source Version** | **Object Version** | **Compatibility** |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |

# Update instructions

Before updating the ADS file, the ADS file need to be renamed and ensured it’s name less than 9 letters.