

SDG5000 Firmware Revision History

Revision History

|  |  |  |
| --- | --- | --- |
| **Date** | **Version** | **Revision** |
| 2/1/2018 | 5.01.01.15R5 | 1. Optimized PLL configuration 2. Fixed several bugs    1. Enabling Mod on CH2 may disable Burst on CH1    2. Duty cycle error on Square wave with very long period    3. SCPI command cannot adjust the phase difference between two synchronized units    4. Manual trigger cannot trigger both channels   simultaneously |
| 11/11/2015 | 5.01.01.15R1 | 1. Supported bandwidth update option （Note: The option will be only available on the hardware after Jan. 1st, 2016） 2. Added channel coupling function 3. Fixed miscellaneous minor bugs |

1 / 1